**Car Scanner** [**ELM327 Bluetooth V2**](https://www.mapout24.com/gps-device/uncategorized/elm327-bluetooth-obdii-auto-car-diagnostic-scanner-android-torque-app/) **Bluetooth Interface**

ELM327 Car Scanner Bluetooth CAN-BUS scan tool supports OBD-II protocols it is used to read & diagnose trouble codes, clear trouble codes and detect fuel pressure and so on. ELM327 Bluetooth Interface Auto Diagnostic OBD #Scanner an on-Board Diagnostics, or OBD, in an automotive context, is a generic term referring to a vehicles self-diagnostic and reporting capability.

**Free** [**Torque App**](https://play.google.com/store/apps/details?id=org.prowl.torque&hl=en_IN&gl=US) **ELM327 Car Scanner Bluetooth V2.1 OBD2**

* Engine RPM
* Calculated Load Value
* Coolant Temperature
* Fuel System Status
* Vehicle Speed
* Short Term Fuel Trim
* Long Term Fuel Trim
* Intake Manifold Pressure
* Timing Advance
* Intake Air Temperature
* Air Flow Rate
* Absolute Throttle Position
* Oxygen sensor voltages/associated short term fuel trims
* Fuel System status
* Fuel Pressure

**ELM327** [**OBD2 V2.1 Bluetooth Interface Auto  #**](https://www.electronicscomp.com/elm327-obd2-v2.1-bluetooth-interface-auto-car-diagnostic-scanner)**Car Scanner**

Car Scanner Elm327 Bluetooth adapter gives you the opportunity to spy on your car wirelessly. Convert your PC, PDA, Mobile to a diagnostic tool and monitor all critical information of the cars ECU. The Car Scanner Elm327 Bluetooth is an adapter that connects to the cars network and then creates a virtual cable between the adapter and the PC that it is connected. With the help of various open source application for the Elm327, you can have a digital gauge or an advanced. diagnostic system and a powerful performance measurement toll in your screen.

1. OBD Car scanner  Read diagnostic trouble codes, both generic and manufacturer-specific, and display their meaning (over 3000 generic code definitions in the database).
2. Clear trouble codes and turn off the MIL (Check Engine light)
3. Supported car scanner : All cars, [Bike](https://www.mapout24.com/can-you-put-an-obd-scanner-in-a-motorcycle/) made after 2009 except listed below
4. Non supported car models : all SVU models , all fiat models , Tata models till 2013, Maruti s coss, sx4 , basic model like maruti 800 , santo , omani will support made after 2013
5. Main function : Read & Remove Engine check light fault code ( ABS , AIR BAG light can't remove by this device

**Car Scanner Specifications :-**

|  |  |
| --- | --- |
| Support OBD-II protocols | ISO15765-4 (CAN) ISO14230-4 (KWP2000) ISO9141-2 J1850 VPW J1850 PWM |
| Color | Back + Orange + Blue |
| Dimensions (LxWxH) mm | 8.2 x 4.6 x 2.5cm |
| Weight(gm) | 45 |